How many grams of NaHCO3 would be required to keep the ANC levels in a lake above 50 µeq/L for 3 hydraulic residence times given an influent pH of 3.0 and a lake volume of 4 L, if the current lake ANC is 0 µeq/L?